!### Step 4 Commands ###!

!### Configuring MG WAN interface###!

en

conf t

hostname MG

int s0/0/0

ip address 209.165.200.18 255.255.255.240

no shut

exit

!### Configuring MG LAN interface###!

int g0/0

ip address 172.16.0.1 255.255.255.0

no shut

exit